|  |
| --- |
| After a fire: using your personal protective kit  Community information |
|  |

Protective kits are for people returning to properties affected by fire. They are available from your local council or an emergency recovery centre, along with additional masks, disposable coveralls and sturdy gloves.

**Kits should only be used for personal protection during property inspections.   
  
They are not for asbestos removal or clean-up.**

The information sheet *After a fire: returning home safely* is included in the kit, which details the health and safety considerations that you should know before re-entering your property.

Each protective kit contains:

* disposable coveralls
* a disposable P2 face mask
* sturdy gloves
* a garbage bag to dispose of used protective equipment

information sheets:

* *After a fire: returning home safely*
* *After a fire: using your personal protective kit.*



How many kits will I need?

As the protective equipment is disposable and should not be re-used, several kits may be required for each person, depending on the time spent at the property.

**Masks, coveralls and gloves should be removed and thrown away:**

* **whenever you break from work**
* **when you leave your property**
* **before entering vehicles.**

Wearing sturdy footwear that can be easily cleaned or washed down when leaving your property is recommended.

How to use the protective equipment:

* Follow the instructions over the page for guidance on fitting the mask – be aware that beards and moustaches prevent men from getting a good seal with masks.

Coveralls should be worn over your clothing.

To remove and dispose of the protective equipment:

* Disposable coveralls should be peeled off inside out and placed in the bag.
* Gloves should be removed and placed in the bag.
* Thoroughly wash down footwear if not being thrown away.
* Remove the face mask last, placing it in the bag.
* Seal the bag tightly by tying a knot.
* Dispose of the bag at any refuse collection point.

Further information

Contact your local council or an emergency recovery centre for more protective kits or if you have questions about using the kit.  
  
Authorised and published by the Victorian Government,   
1 Treasury Place, Melbourne.

© State of Victoria, Department of Health and Human Services, February 2016.

How to put on and fit check a **P2** or **N95** mask



**1**

**2**

**3**

**4**

**5**

**6**

**7**

**8**

**9**

**10**

**11**

**12**

Bend the nose wire to form a gentle curve. The nose wire represents the top of the mask

Separate the edges of the mask to fully open it

Hold the mask upside down to expose the two straps

Using your index fingers and thumbs, separate the two straps

While holding the straps, cup the mask under your chin

Pull the straps up and over your head

Place and position the lower strap at the base of your neck (under your ears)

Place the upper strap on the crown of your head so that it runs just above the top of your ears

Gently press the nose wire down across the bridge of your nose until it fits snugly

Continue to adjust the mask and edges until you feel you have achieved a good and comfortable fit

**FIT CHECK**

Gently inhale. When you breathe in the mask should draw in slightly toward the face and collapse

Follow these directions each time the mask is worn. The masks will not provide the intended level of protection unless worn correctly so it is important that you achieve a good fit as detailed above. Men who are clean shaven will achieve the best facial seal. The brand of P2 or N95 masks may vary slightly so always follow the manufacturer’s instructions and warnings.

Gently exhale. The mask should fill up with air. It is important at this stage that there is no air leakage around edges of mask.

**A ‘fit check’ must be performed each time a P2 or N95 mask is worn**